Power Wheel Class  
POWERWHEELS AGES 4-10  
1. The stock battery can be replaced with a 12-volt mower battery only, it can be positioned anywhere inside the car and covered. Not in the passenger seat.  
2. Secure the doors and hoods with a bungy cord or rope so they don't come open. 
3. Seatbelts are not mandatory but recommended, helmets are mandatory though. 4. Any rollover bars will be allowed if we feel they are safe and don't reinforce the cars. Bring your saws. 5. You can put screws in tires for traction if it is safe.  
6. DO NOT make the power wheels go any faster than the factory or you will not be permitted to run. ALL POWER WHEELS MUST SIT LIKE THE STORE-BOUGHT ONES NO RAISING OR LOWERING THE FRONT OR REAR OF THE POWER WHEELS SCREWS MAY BE ADDED TO TIRES FOR TRACTION. 

